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DJI MINI MICROPHONE CONNECTION GUIDE

	


Connect the DJI wireless microphone to the CFE Lightboard PC before opening eGlass Fusion.
	1. TURN ON THE MICROPHONE


	[image: Photograph showing a DJI microphone charging case resting on a dark carrying bag atop a table. Red arrow and label identify case, with papers, window, and green bottle visible in background.]
	Open the DJI charging case, remove the microphone, and press the Power button to turn it on.


	2. PAIR THE MICROPHONE WITH THE LIGHTBOARD PC


	[image: Photograph of a compact wireless microphone transmitter with furry windscreen, showing labeled power and Bluetooth buttons. Red arrows identify controls, while a green status light indicates blue pairing mode.]
	A. Put the microphone in pairing mode
Press and hold the Bluetooth button until the status light turns blue.
B. Connect in Windows
· Open Settings > Bluetooth & devices.
· Choose Add device > Bluetooth.
· Select the DJI microphone when it appears.


	3. SELECT THE DJI MICROPHONE IN EGLASS


· Open eGlass Fusion, go to Settings, and select the DJI microphone as the microphone/audio input.
	If eGlass is already open and you do not see the DJI option, close eGlass and open it again.

	4. TEST BEFORE RECORDING


· Record a short test video and play it back to confirm the microphone is working.
· When finished, turn off the microphone and return it to the charging case.
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